EL 2003 Comp Org & Assembly Language Lab

LABORATORY MANUAL ⦁Fall 2022⦁Instructor:Rukhsar Ali

|  |
| --- |
| **LAB 04** |

**Flags & Data Related Operations**

****

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | | | | |
|  | | | | |
|  | | | | |
|  | |  | |  |
| \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | \_\_\_\_\_\_\_\_\_\_ | | \_\_\_ |
| STUDENT NAME | | ROLL NO | | SEC |
|  | | | | |
| \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | | | |
| SIGNATURE & DATE | | | | |
| **MARKS AWARDED: \_\_\_\_\_\_\_\_\_\_\_\_\_\_** | | | | |
| \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | | | |
| **NATIONAL UNIVERSITY OF COMPUTER AND EMERGING SCIENCES (NUCES), KARACHI** | | | | |
|  | | | | |
| Prepared by: | Rukhsar Ali |  |  | |

**Lab Session 04: Flags & Data Related Operations**

**Objectives:**

* Observing effect of Arithmetic Instructions on Flag Register
* Direct-offset operands
* OFFSET operator
* PTR operator
* TYPE operator
* LENGTHOF operator
* SIZEOF operator
* Indirect operands
* Indexed operands

**Arithmetic Instructions & Flags**

Status flags are updated to indicate certain properties of the result. Once a flag is set, it remains in that state until another instruction that affects (update) the flags is executed.

**\*NOTE:** A flag is set when it equals to 1, otherwise it is clear

**Z-Zero Flag:**

The Zero flag is set when the result of an operation produces zero in the destination operand.

mov cx , 1

sub cx , 1 ; CX=0, ZF=1

mov ax , 0FFFFh

inc ax ; AX=0, ZF=1;

inc ax ; AX=1, ZF=0;

**C-Carry Flag:**

This flag is set, when there is a carry out of MSB in case of addition and borrow in case of subtraction. The Carry flag is set when the result of an operation generates an unsigned value that is out of range (too big or too small for the destination operand).

mov al , 0FFh

add al , 1 ;CF=1, AL=0

; for trying less than 0

sub al , 1 ; CF=1, AL=FF

**S-Sign Flag:**

This flag indicates the sign of the result of an operation. A 0 for positive number and 1 for a negative number.

mov al , 15

add al , 97 ;observe SIGN Flag

mov al , 15

sub al , 97 ;observe SIGN Flag

mov al , 97

add al , 97 ;observe SIGN Flag

**AC-Auxilary Carry Flag:**

This flag is set, if there is a carry from the lowest nibble, i.e., bit three during addition, or borrow for the lowest nibble, i.e. bit three, during subtraction.

Suppose we add 1 to 0Fh. The sum (10h) contains a 1 in bit position 4 that was carried out of bit position 3:

mov al , 0Fh

add al , 1 ;AC=1

**P Parity Flag:**

The Parity flag (PF) is set when the least significant byte of the destination has an even number of 1 bits. The following ADD and SUB instructions alter the parity of AL:

mov al , 10001100b

add al , 000000010b ; AL=10001110, PF =1

sub al , 100000000b ; AL=00001110, PF = 0

**O-Over flow Flag:**

The Overflow flag is set when the result of a signed arithmetic operation over-flows or underflows the destination operand. For example, the largest possible integer signed byte value is

+127; adding 1 to it causes overflow:

mov al , 127

add al , 1 ; OF=1

Similarly, the smallest possible negative integer byte value is 128. Subtracting 1 from it causes underflow. The destination operand value does not hold a valid arithmetic result, and the Over- flow flag is set:

mov al , -128

sub al , 1 ; OF=1

**DATA Related Operations**

**Direct-offset Operands:**

You can add a displacement to the name of a variable, creating a direct-offset operand.

**Example:**

.data

arrayB BYTE 10h,20h,30h,40h,50h

arrayW WORD 100h,200h,300h

.code

mov al,arrayB ; AL = 10h

mov al,[arrayB+1] ; AL = 20h

mov ax,arrayW ; AX = 100h

mov ax,[arrayW+2] ; AX = 200h

**OFFSET Operator:**

The OFFSET operator returns the offset of a data label.

**Syntax:**

MOV reg32, OFFSET mem ; reg32 points to count

**Example:**

.data

bVal BYTE ?

wVal WORD ?

dVal DWORD ?

dVal2 DWORD ?

;If bVal is located at offset 00404000h, we would get:

mov esi, OFFSET bval ; ESI = 00404000

mov esi, OFFSET wVal ; ESI = 00404001

mov esi, OFFSET dVal ; ESI = 00404003

mov esi, OFFSET dVal2 ; ESI = 00404007

**PTR Operator:**

We can use the PTR operator to override the declared size of an operand. Note PTR must be used in combination with one of the standard assembler data types.

**For example:** that we would like to move the lower 16 bits of a doubleword variable named myDouble into AX. The assembler will not permit the following move because the operand sizes do not match:

.data

myDouble DWORD 12345678h

.code

mov ax, myDouble ; error

But the WORD PTR operator makes it possible to move the low-order word (5678h) to AX:

mov ax, word ptr myDouble ; AX = 5678H

and higher word (1234h) to AX:

mov dx, word ptr myDouble+2 ; DX = 1234H

Moving Smaller Values into Larger Destinations

We might want to move two smaller values from memory to a larger destination operand. In the next example, the first word is copied to the lower half of EAX and the second word is copied to the upper half.

The DWORD PTR operator makes this possible:

.data

wordList WORD 5678h, 1234h

.code

mov eax, DWORD PTR wordList ; EAX = 12345678h

**TYPE Operator:**

The TYPE operator returns the size, in bytes, of a single element of a variable.

Syntax:

MOV reg16, TYPE mem

**Example 1:**

.data

var1 BYTE ? ; TYPE var1 = 1

var2 WORD ? ; TYPE var2 = 2

var3 DWORD ? ; TYPE var3 = 4

var4 QWORD ? ; TYPE var4 = 8

**Example 2:**

.data

var1 BYTE 20h

var2 WORD 1000h

var3 DWORD ?

var4 BYTE 10, 20, 30, 40, 50

msg BYTE ‘File not found’, 0

.code

mov ax, type var1 ; AX = 0001

mov ax, type var2 ; AX = 0002

mov ax, type var3 ; AX = 0004

mov ax, type var4 ; AX = 0001

mov ax, type msg ; AX = 0001

**LENGTHOF Operator:**

The LENGTHOF operator counts the number of individual elements in a variable that has been defined using DUP.

Syntax:

MOV reg16 , LENGTHOF mem

**Example:**

.data

val1 WORD 1000h

val2 SWORD 10, 20, 30 array WORD 10 DUP(?),0

array2 WORD 5 DUP(3 DUP(0))

message BYTE ‘File not found’, 0

.code

mov ax, LENGTHOF val1 ; AX = 1

mov ax, LENGTHOF val2 ; AX = 3

mov ax, LENGTHOF array ; AX = 11

mov ax, LENGTHOF array2 ; AX = 15

mov ax, LENGTHOF message ; AX = 15

**SIZEOF Operator:**

The SIZEOF operator returns the number of bytes an array takes up. It is similar in effect to multiplying LENGTHOF with TYPE.

Syntax:

MOV reg16/32 , SIZEOF mem

**Example:**

.data

intArray WORD 32 DUP(0)

.code

mov eax,SIZEOF intArray ; EAX = 64

**Indirect Operands**

In protected mode, an indirect operand can be any 32-bit general-purpose register (EAX, EBX, ECX, EDX, ESI, EDI, EBP, and ESP) surrounded by brackets. The register is assumed to contain the address of some data.

**Example:**

.data

byteVal BYTE 10h

.code

mov esi,OFFSET byteVal

mov al,[esi] ; AL = 10h

If the destination operand uses indirect addressing, a new value is placed in memory at the location pointed to by the register.

mov [esi],bl

Using PTR with Indirect Operands

inc [esi] ; error: operand must have size

The assembler does not know whether ESI points to a byte, word, doubleword, or some other size. The PTR operator confirms the operand size:

inc BYTE PTR [esi]

**Arrays**

Indirect operands are ideal tools for stepping through arrays.

**Example:**

.data

arrayB BYTE 10h,20h,30h

.code

mov esi,OFFSET arrayB

mov al,[esi] ; AL = 10h

inc esi

mov al,[esi] ; AL = 20h

If we use an array of 16-bit integers, we add 2 to ESI to address each subsequent array element.

.data

arrayW WORD 1000h,2000h,3000h

.code

mov esi,OFFSET arrayW

mov ax,[esi] ; AX = 1000h

add esi,2

mov ax,[esi] ; AX = 2000h

If we use an array of 32-bit integers, we add 4 to ESI to address each subsequent array element.

**Indexed Operands**

An indexed operand adds a constant to a register to generate an effective address. Any of the 32-bit general-purpose registers may be used as index registers.

Syntax:

constant [ reg32 ] ; reg32 can be any of the 32-bit general registers

[ constant + reg32 ]

**Example:**

.data

arrayB BYTE 20, 40, 60, 80

.code

mov esi, 1

mov al, arrayB[esi]

inc esi

mov al, arrayB[esi]

mov esi, 3

mov al, [arrayB + esi]

Adding Displacements: The second type of indexed addressing combines a register with a constant offset. The index register holds the base address of an array.

.data

arrayW WORD 1000h,2000h,3000h

.code

main PROC

mov esi,OFFSET arrayW

mov ax,[esi] ; AX = 1000h

mov bx,[esi+2] ; BX = 2000h

mov cx,[esi+4] ; CX = 3000h

**Scale Factors in Indexed Operands**

Indexed operands must take into account the size of each array element when calculating offsets.

Syntax:

constant [ reg32 \* TYPE constant]

**Example:**

.data

arrayW WORD 1000h, 2000h, 3000h, 4000h

.code

main PROC

mov eax,0

mov ebx,0

mov ecx,0

mov esi, 1

mov ax, arrayW[esi \* TYPE arrayW]

mov esi, 2

mov bx, arrayW[esi \* TYPE arrayW]

mov esi, 3

mov cx, arrayW[esi \* TYPE arrayW]

call DumpRegs

**Lab Exercise:**

1. Declare a 32-bit signed integer **val1** and initialize it with the 8000h. If **val1** is incremented by 1000h using the ADD instruction, what will be the values of the Carry and Sign flags?
2. Write down the values of the Carry, Sign, Zero, and Overflow flags after each instruction has executed:

mov ax , 7FF0h ;CF=?, SF=?, ZF=?, OF=?

add al , 10h ;CF=?, SF=?, ZF=?, OF=?

add ah , 1 ;CF=?, SF=?, ZF=?, OF=?

add ax , 2 ;CF=?, SF=?, ZF=?, OF=?

1. Initialize a double word array consisting of elements 8, 5, 1, 2 ,6. Re-arrange the given array in ascending order directly with the help of registers. Use direct-offset addressing to access the elements.
2. Use following array declarations:

arrayB BYTE 10, 20, 30

arrayW WORD 150, 250, 350

arrayD DWORD 600, 1200, 1800

Now initialize three double word variables SUM1, SUM2, SUM3 and perform following operations (expressed in pseudo-code here):

SUM1 = arrayB[0] + arrayW[0] + arrayD[0]

SUM2 = arrayB[1] + arrayW[1] + arrayD[1]

SUM3 = arrayB[2] + arrayW[2] + arrayD[2]

**\*HINT:** Use movzx instruction.

1. Initialize two arrays:

array1 BYTE 10, 20, 30, 40

array2 BYTE 4 DUP (?)

Copy elements of array1 into array2 in reverse order using either indirect addressing or direct-offset addressing.

1. Create an array of 5 doublewords and subtract remaining all elements of array from 1st element using indirect operands.
2. Use following array declarations:

arrayB BYTE 60, 70, 80

arrayW WORD 150, 250, 350

arrayD DWORD 600, 1200, 1800

For each array, add its 1st and last element using scale factors and display the result in a separate register.